(export (version "E")
  (design
    (source "/home/yann/Documents/Projet/Reveil/PCB/Boutons/PCBBoutons/PCBBoutons.kicad_sch")
    (date "2025-08-23T17:54:38+0200")
    (tool "Eeschema 9.0.2+dfsg-1")
    (sheet (number "1") (name "/") (tstamps "/")
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "PCBBoutons.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value "")))))
  (components
    (comp (ref "J1")
      (value "Conn_01x06_Socket")
      (footprint "Connector_JST:JST_XH_S6B-XH-A-1_1x06_P2.50mm_Horizontal")
      (description "Generic connector, single row, 01x06, script generated")
      (fields
        (field (name "Footprint") "Connector_JST:JST_XH_S6B-XH-A-1_1x06_P2.50mm_Horizontal")
        (field (name "Datasheet"))
        (field (name "Description") "Generic connector, single row, 01x06, script generated"))
      (libsource (lib "Connector") (part "Conn_01x06_Socket") (description "Generic connector, single row, 01x06, script generated"))
      (property (name "Sheetname") (value "Racine"))
      (property (name "Sheetfile") (value "PCBBoutons.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "d7ab2f41-45a1-45d3-86b6-ce58274af17b"))
    (comp (ref "R1")
      (value "R")
      (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal")
      (description "Resistor")
      (fields
        (field (name "Footprint") "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal")
        (field (name "Datasheet"))
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Racine"))
      (property (name "Sheetfile") (value "PCBBoutons.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "79b06aa7-2f49-49ce-a2f3-61366ebd8f5c"))
    (comp (ref "R2")
      (value "R")
      (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal")
      (description "Resistor")
      (fields
        (field (name "Footprint") "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal")
        (field (name "Datasheet"))
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Racine"))
      (property (name "Sheetfile") (value "PCBBoutons.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "ef5d926b-f7be-4d06-b712-82faad2bfffd"))
    (comp (ref "R3")
      (value "R")
      (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal")
      (description "Resistor")
      (fields
        (field (name "Footprint") "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal")
        (field (name "Datasheet"))
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Racine"))
      (property (name "Sheetfile") (value "PCBBoutons.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "cc1440c0-1dc2-4540-a29f-12ac0ead3784"))
    (comp (ref "R4")
      (value "R")
      (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal")
      (description "Resistor")
      (fields
        (field (name "Footprint") "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal")
        (field (name "Datasheet"))
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Racine"))
      (property (name "Sheetfile") (value "PCBBoutons.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "fabc8c51-1fbc-4719-8284-dade725eb453"))
    (comp (ref "SW1")
      (value "SW_Push")
      (footprint "Button_Switch_THT:SW_PUSH_6mm")
      (description "Push button switch, generic, two pins")
      (fields
        (field (name "Footprint") "Button_Switch_THT:SW_PUSH_6mm")
        (field (name "Datasheet"))
        (field (name "Description") "Push button switch, generic, two pins"))
      (libsource (lib "Switch") (part "SW_Push") (description "Push button switch, generic, two pins"))
      (property (name "Sheetname") (value "Racine"))
      (property (name "Sheetfile") (value "PCBBoutons.kicad_sch"))
      (property (name "ki_keywords") (value "switch normally-open pushbutton push-button"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "6938a97b-81a5-4e26-adbe-acb265b51f16"))
    (comp (ref "SW2")
      (value "SW_Push")
      (footprint "Button_Switch_THT:SW_PUSH_6mm")
      (description "Push button switch, generic, two pins")
      (fields
        (field (name "Footprint") "Button_Switch_THT:SW_PUSH_6mm")
        (field (name "Datasheet"))
        (field (name "Description") "Push button switch, generic, two pins"))
      (libsource (lib "Switch") (part "SW_Push") (description "Push button switch, generic, two pins"))
      (property (name "Sheetname") (value "Racine"))
      (property (name "Sheetfile") (value "PCBBoutons.kicad_sch"))
      (property (name "ki_keywords") (value "switch normally-open pushbutton push-button"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "053f6181-c7cf-4f7a-a8dd-0129c75064e4"))
    (comp (ref "SW3")
      (value "SW_Push")
      (footprint "Button_Switch_THT:SW_PUSH_6mm")
      (description "Push button switch, generic, two pins")
      (fields
        (field (name "Footprint") "Button_Switch_THT:SW_PUSH_6mm")
        (field (name "Datasheet"))
        (field (name "Description") "Push button switch, generic, two pins"))
      (libsource (lib "Switch") (part "SW_Push") (description "Push button switch, generic, two pins"))
      (property (name "Sheetname") (value "Racine"))
      (property (name "Sheetfile") (value "PCBBoutons.kicad_sch"))
      (property (name "ki_keywords") (value "switch normally-open pushbutton push-button"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "fc5128f8-11e1-4737-8036-4ed9d5651ac3"))
    (comp (ref "SW4")
      (value "SW_Push")
      (footprint "Button_Switch_THT:SW_PUSH_6mm")
      (description "Push button switch, generic, two pins")
      (fields
        (field (name "Footprint") "Button_Switch_THT:SW_PUSH_6mm")
        (field (name "Datasheet"))
        (field (name "Description") "Push button switch, generic, two pins"))
      (libsource (lib "Switch") (part "SW_Push") (description "Push button switch, generic, two pins"))
      (property (name "Sheetname") (value "Racine"))
      (property (name "Sheetfile") (value "PCBBoutons.kicad_sch"))
      (property (name "ki_keywords") (value "switch normally-open pushbutton push-button"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "2988a082-0acd-401c-9d78-98f12f441417")))
  (libparts
    (libpart (lib "Connector") (part "Conn_01x06_Socket")
      (description "Generic connector, single row, 01x06, script generated")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x06_Socket")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x06, script generated"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))
        (pin (num "5") (name "Pin_5") (type "passive"))
        (pin (num "6") (name "Pin_6") (type "passive"))))
    (libpart (lib "Device") (part "R")
      (description "Resistor")
      (docs "~")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "R")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Switch") (part "SW_Push")
      (description "Push button switch, generic, two pins")
      (docs "~")
      (fields
        (field (name "Reference") "SW")
        (field (name "Value") "SW_Push")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Push button switch, generic, two pins"))
      (pins
        (pin (num "1") (name "1") (type "passive"))
        (pin (num "2") (name "2") (type "passive")))))
  (libraries
    (library (logical "Connector")
      (uri "/usr/share/kicad/symbols//Connector.kicad_sym"))
    (library (logical "Device")
      (uri "/usr/share/kicad/symbols//Device.kicad_sym"))
    (library (logical "Switch")
      (uri "/usr/share/kicad/symbols//Switch.kicad_sym")))
  (nets
    (net (code "1") (name "+3.3V") (class "Default")
      (node (ref "J1") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "SW1") (pin "2") (pinfunction "2") (pintype "passive"))
      (node (ref "SW2") (pin "2") (pinfunction "2") (pintype "passive"))
      (node (ref "SW3") (pin "2") (pinfunction "2") (pintype "passive"))
      (node (ref "SW4") (pin "2") (pinfunction "2") (pintype "passive")))
    (net (code "2") (name "GND") (class "Default")
      (node (ref "J1") (pin "6") (pinfunction "Pin_6") (pintype "passive"))
      (node (ref "R1") (pin "1") (pintype "passive"))
      (node (ref "R2") (pin "1") (pintype "passive"))
      (node (ref "R3") (pin "2") (pintype "passive"))
      (node (ref "R4") (pin "1") (pintype "passive")))
    (net (code "3") (name "Net-(J1-Pin_2)") (class "Default")
      (node (ref "J1") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "R1") (pin "2") (pintype "passive"))
      (node (ref "SW1") (pin "1") (pinfunction "1") (pintype "passive")))
    (net (code "4") (name "Net-(J1-Pin_3)") (class "Default")
      (node (ref "J1") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "R2") (pin "2") (pintype "passive"))
      (node (ref "SW2") (pin "1") (pinfunction "1") (pintype "passive")))
    (net (code "5") (name "Net-(J1-Pin_4)") (class "Default")
      (node (ref "J1") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "R3") (pin "1") (pintype "passive"))
      (node (ref "SW3") (pin "1") (pinfunction "1") (pintype "passive")))
    (net (code "6") (name "Net-(J1-Pin_5)") (class "Default")
      (node (ref "J1") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "R4") (pin "2") (pintype "passive"))
      (node (ref "SW4") (pin "1") (pinfunction "1") (pintype "passive")))))