
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "ESP32-S3-DEVKITC-1-N8R2" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -17.78 35.56 0)
      (effects (font (size 1.27 1.27)) (justify top left))
    )
    (property "Value" "ESP32-S3-DEVKITC-1-N8R2" (id 1) (at -17.78 -35.56 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "ESP32-S3-DEVKITC-1-N8R2:XCVR_ESP32-S3-DEVKITC-1-N8R2" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "Espressif Systems" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n                        \n                            WiFi Development Tools - 802.11 ESP32-S3 general-purpose development board, embeds ESP32-S3-WROOM-1-N8R2, with pin header\n                        \n" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "None" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "None" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/ESP32-S3-DEVKITC-1-N8R2/Espressif+Systems/view-part/?ref=eda" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "V1" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/ESP32-S3-DEVKITC-1-N8R2/Espressif+Systems/view-part/?ref=snap" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "ESP32-S3-DEVKITC-1-N8R2" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "In Stock" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Espressif" (id 14) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "ESP32-S3-DEVKITC-1-N8R2_0_0"
      (rectangle (start -17.78 -33.02) (end 17.78 33.02)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin power_in line (at 22.86 27.94 180.0) (length 5.08)
        (name "3V3"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 22.86 27.94 180.0) (length 5.08)
        (name "3V3"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -22.86 25.4 0) (length 5.08)
        (name "RST"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 17.78 0) (length 5.08)
        (name "GPIO1"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 15.24 0) (length 5.08)
        (name "GPIO2"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 10.16 0) (length 5.08)
        (name "GPIO4"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 12.7 0) (length 5.08)
        (name "GPIO3"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_13"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 7.62 0) (length 5.08)
        (name "GPIO5"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 5.08 0) (length 5.08)
        (name "GPIO6"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 2.54 0) (length 5.08)
        (name "GPIO7"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 0.0 0) (length 5.08)
        (name "GPIO8"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 -2.54 0) (length 5.08)
        (name "GPIO9"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_15"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 -5.08 0) (length 5.08)
        (name "GPIO10"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_16"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 -7.62 0) (length 5.08)
        (name "GPIO11"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_17"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 -10.16 0) (length 5.08)
        (name "GPIO12"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_18"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 -12.7 0) (length 5.08)
        (name "GPIO13"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_19"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 -15.24 0) (length 5.08)
        (name "GPIO14"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_20"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 -17.78 0) (length 5.08)
        (name "GPIO15"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 -20.32 0) (length 5.08)
        (name "GPIO16"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 -22.86 0) (length 5.08)
        (name "GPIO17"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_10"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 -25.4 0) (length 5.08)
        (name "GPIO18"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_11"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 20.32 0) (length 5.08)
        (name "GPIO0"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_14"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 22.86 -30.48 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_22"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 22.86 -30.48 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 22.86 -30.48 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_21"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 22.86 -30.48 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_22"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 22.86 30.48 180.0) (length 5.08)
        (name "5V0"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_21"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 2.54 180.0) (length 5.08)
        (name "GPIO48"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_16"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 5.08 180.0) (length 5.08)
        (name "GPIO47"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_17"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 7.62 180.0) (length 5.08)
        (name "GPIO46"
          (effects (font (size 1.016 1.016)))
        )
        (number "J1_14"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 10.16 180.0) (length 5.08)
        (name "GPIO45"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_15"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -22.86 -27.94 0) (length 5.08)
        (name "GPIO21"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_18"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 -25.4 180.0) (length 5.08)
        (name "USB_D+/GPIO20"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_19"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 -22.86 180.0) (length 5.08)
        (name "USB_D-/GPIO19"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_20"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 -17.78 180.0) (length 5.08)
        (name "U0RXD/GPIO44"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 -15.24 180.0) (length 5.08)
        (name "U0TXD/GPIO43"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 -10.16 180.0) (length 5.08)
        (name "MTMS/GPIO42"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 -7.62 180.0) (length 5.08)
        (name "MTDI/GPIO41"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 -5.08 180.0) (length 5.08)
        (name "MTDO/GPIO40"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 -2.54 180.0) (length 5.08)
        (name "MTCK/GPIO39"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 12.7 180.0) (length 5.08)
        (name "GPIO38"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_10"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 15.24 180.0) (length 5.08)
        (name "GPIO37"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_11"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 17.78 180.0) (length 5.08)
        (name "GPIO36"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 22.86 20.32 180.0) (length 5.08)
        (name "GPIO35"
          (effects (font (size 1.016 1.016)))
        )
        (number "J3_13"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)